Roba Profi Clean
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• Backside cleaning of thermo foiled doors

• Cleaning of laminated furniture panels

The Roba Profi Clean as through feed solution

guarantees high productivity with best cleaning

results.
Advantages of the

Roba Profi Clean principle:
•  Optimized cleaning from dust and glue residues

•  Optimal rounding of sharp edges
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work clock- and counter-

clockwise,equipped with 
special cotton brushes for

secure cleaning.
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The Roba Profi Clean 
is suitable for cleaning 
of all kind of laminated  
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furniture parts

Technical information:  Roba Profi Clean 1300

cleaning machine for laminated surfaces, consisting of:

1 pc.:
Stable base frame for mounting

         
the sanding units in encapsulated version.

1 pc.: 
Conveyor belt with 1300mm working width,

        
With drive and tensioning station in solid construction. 

Feed electronically infinitely variable

          
from 4 - 15 m/min (13 - 49ft/min), 0,55 KW

2 pc.:  
Double brush cleaning unit for

          
top working in two directions:

         
1st drum clockwise rotation, 2nd drum counter clockwise rotation

          
Cleaning brush diameter:          approx. 250mm (9,8'')

          
Number of segments:               approx. 84 pc./drum

         
Brush width:                             1320 mm (51,2'')

          
Special cotton brushes for best cleaning results.

          
Drive: 3,0 KW each gearbox i=1:2

         
electronically infinitely variable from 200 -700 rpm

         
Linear-guided, workpiece thicknesses adjustable

         
with spindle from 5-80 mm (0,2-3,15'').

         
Manually adjustable using digital counter

         
Extraction hood diameter: 160 mm  (6,3'')

1 pc.:
Cleaning unit with blower system at machine exit

2 pc.: 
Top pressure system with 3 pieces rubberized pressure roller at entrance, exit and centre of double brush unit.

Machine data:
Machine weight:
approx.1800 kg

Machine length: 
approx.2520 mm (99'')

Machine width:  
approx.1940 mm (76'')

Machine height: 
approx.2050 mm (81'')

Working height:      

  900 + / - 50 mm  (35,4'')

Working width: 

1300 mm  (51,2'')

Input power:     

13 KW

Electrical equipment:
central control and switchgear cabinet IB54 protected

as console version.

Operation side on the left in transportation direction.

Operational Voltage EU:230-400V /3PH/N 50Hz.
Or

Operational Voltage US: : 3-phase 460-480V, 60Hz

Electrical components:
The electrical equipment of cabinet components will be done according to UL/CSA/CUS standards. All electrical devices of the plant are UL/CSA/CUS approved.

The high standards used for manufacturing the plant will comply with CE standards.

Delivery will be done with EU normed wiring diagrams.

Operating voltage: 3-phase 460-480V, 60Hz 

Permissible mains types: All TT systems, TN systems or systems with grounded star 

point without additional measures is permitted.

Operating at IT systems is not allowed and will destroy electrical components.

There is no UL/CSA/CUS certification sticker provided with 

the machine. 

Inverter:                        
Schneider Electric

Gearbox:                   

Getriebebau Nord

Displays and controls:  
Klöckner Möller

Machine CE certification

Machine colour:              
RAL 7035

Safety cover colour:     
RAL 5018

Optional:

1 pc.:   Motorized height positioning per unit

Cleaning method





The Roba Profi Clean machine line guarantees as a through feed solution high productivity. As a stand-alone solution for large quantities or directly behind the turnover/backside trimming


equipment of a thermofoiling line. The only solution that is able to feed a complete batch of doors coming out of a membrane press. During this operation the laminated fronts get cleaned from glue residues and simultaneously


all four edges are slightly rounded without the risk of delamination. Therefore the parts do not require any further processing steps and can be forwarded directly to the packaging. This is


ensured by two or four clockwise and counterclockwise working cleaning drums, which are equipped with special cotton brushes. Further on this machine is also able to show its high capability in the cleaning of all other laminated


furniture parts. 





Roba Profi Clean equipped


with two double brush 


cleaning aggregates








